; SoundMAX device information file.
; Analog Devices, Inc. Copyright(c) 1998 - 2000

[Version]
Signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
provider=%ANLG%
DriverVer = 03/20/2000,5.12.01.2502
;CatalogFile=smx.cat

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MfgName%=AnalogDevices

[AnalogDevices]
;
; You must add the appropriate PnP identifiers for your particular system here.
;
;%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_AAAA&subsys_xxxxyyyy
;
; Replace AAAA with the appropriate I/O Controller Hub ID.
;               2415 for ICH  (82801AA)
;               2425 for ICH1 (82801AB)
;               2445 for ICH2 (82801BA)
;               7195 for Mobile Platform (Bannister)
;
; Replace xxxx with your unique Subsystem ID
;
; Replace yyyy with your Subsystem Vendor ID (PCI Sig ID)
;
;
; NOTE: The following are used by Analog Devices, Inc.
%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_2415&subsys_104311D4

%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_2425&subsys_104311D4
%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_2425&subsys_11D41043
%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_2445&subsys_104311D4

%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_7195&subsys_104311D4
%*WDM_ICHAUD.DeviceDesc%=WDM_ICHAUD, pci\ven_8086&dev_7195&subsys_11D41043


[DestinationDirs]
DefaultDestDir = 10,system32\drivers   ; %SystemRoot%\system32\drivers
WDM_ICHAUD.CopyList = 10,system32\drivers   ; %SystemRoot%\system32\drivers

[WDM_ICHAUD]
DriverVer = 03/20/2000,5.12.01.2502
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=WDM_ICHAUD.CopyList
DelFiles=system.DelFiles
AddReg=WDM_ICHAUD.AddReg, WDM_ICHAUD_GUID.AddReg, DriverInfo.AddReg

[WDM_ICHAUD.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, ICHAud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, ICHAud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, ICHAud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, ICHAud.Interface.Topology

[WDM_ICHAUD.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,smwdm.sys
HKR,,NTMPDriver,,"smwdm.sys,sbemul.sys"

HKR,Drivers,SubClasses,,"wave,midi,mixer"

HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv, Description,,%*WDM_ICHAUD.DeviceDesc%
HKR,Drivers\midi\wdmaud.drv, Description,,%WDM_MIDI%
HKR,Drivers\mixer\wdmaud.drv,Description,,%*WDM_ICHAUD.DeviceDesc%

; Establish max/min values for Volume nodes. "xxxxMax" is the setting for
;  maximum volume level (minimum attenuation). "xxxxMin" is the setting for
;  minimum volume level (maximum attenuation). These values are the Max/Min
;  bits written to the register for the Max/Min level. As an example, the
;  MicIn maximum volume can be set to 2 which equals a maximum output of +9 db,
;  the MicIn minimum is set to 10 which equals a minimum output of - 12 db.
;  (All register values are Hex.)
;

;HKR, Settings, "MasVMax", 1, 00  ;   Master Volume
;HKR, Settings, "MasVMin", 1, 3F  ;
HKR, Settings, "HP_VMax", 1, 06  ;   Headphone Volume
;HKR, Settings, "HP_VMin", 1, 10  ;
HKR, Settings, "MicVMax", 1, 02  ;   Mic In Volume
HKR, Settings, "MicVMin", 1, 10  ;
;HKR, Settings, "PCBVMax", 1, 00  ;   PCBeep Volume
;HKR, Settings, "PCBVMin", 1, 1f  ;
;HKR, Settings, "PhoVMax", 1, 00  ;   Phone Volume
;HKR, Settings, "PhoVMin", 1, 1f  ;
;HKR, Settings, "LinVMax", 1, 00  ;   LineIn Volume
;HKR, Settings, "LinVMin", 1, 1f  ;
;HKR, Settings, "VidVMax", 1, 00  ;   Video Volume
;HKR, Settings, "VidVMin", 1, 1f  ;
;HKR, Settings, "AuxVMax", 1, 00  ;   Aux Volume
;HKR, Settings, "AuxVMin", 1, 1f  ;
;HKR, Settings, "ACDVMax", 1, 00  ;   Analog CD Volume (not digital redbook !)
;HKR, Settings, "ACDVMin", 1, 1f  ;
;HKR, Settings, "MonVMax", 1, 00  ;   Mono Out Volume
;HKR, Settings, "MonVMin", 1, 1f  ;

; Max/Min record levels. xxxRMax is the maximum gain code for that record
;  source. xxxRMin is the minimum gain code for that source.
;HKR, Settings, "MicRMax", 1, 0F  ;   Mic
;HKR, Settings, "MicRMin", 1, 00  ;
;HKR, Settings, "ACDRMax", 1, 0F  ;   CD (Analog CD, not Redbook Audio)
;HKR, Settings, "ACDRMin", 1, 00  ;
;HKR, Settings, "VidRMax", 1, 0F  ;   Video
;HKR, Settings, "VidRMin", 1, 00  ;
;HKR, Settings, "AuxRMax", 1, 0F  ;   Aux
;HKR, Settings, "AuxRMin", 1, 00  ;
;HKR, Settings, "LinRMax", 1, 0F  ;   Line In
;HKR, Settings, "LinRMin", 1, 00  ;
;HKR, Settings, "OutRMax", 1, 0F  ;   Line output loopback
;HKR, Settings, "OutRMin", 1, 00  ;
;HKR, Settings, "MonRMax", 1, 0F  ;   Mono output loopback
;HKR, Settings, "MonRMin", 1, 00  ;
;HKR, Settings, "PhoRMax", 1, 0F  ;   Phone
;HKR, Settings, "PhoRMin", 1, 00  ;


; Default volume / mute settings. These are the initial installation settings.
; The volume default values are tested againts the Max/Min values that may have
;  been previously established. The Boolean settings (Mute, 20 db, etc.) are
;  set as 0 = FALSE, non-zero = TRUE;
;
; Note that a particular hardware platform may not implement all signal paths.
;
; This is the mixed digital PCM stream (Wave, SW Synth and Digital Redbook)
; This setting is not adjustable from a Mixer control slider. This is
; not adjustable from the Mixer applet.
HKR, Settings, "PCMOutVolume", 1, 07 ;   PCM Out volume 8 = 0db gain, 7 = +1.5db

HKR, Settings, "NULL", 1, 00     ;   Generic handler for un-named nodes

HKR, Settings, "MasV", 1, 08     ;   Master Volume
HKR, Settings, "MasM", 1, 00     ;   Master Mute

HKR, Settings, "PCBV", 1, 08     ;   PCBeep Volume
HKR, Settings, "PCBM", 1, 01     ;   PCBeep Mute

HKR, Settings, "PhoV", 1, 08     ;   Phone Volume
HKR, Settings, "PhoM", 1, 01     ;   Phone Mute

HKR, Settings, "LinV", 1, 08     ;   LineIn Volume
HKR, Settings, "LinM", 1, 01     ;   LineIn Mute

HKR, Settings, "VidV", 1, 08     ;   Video Volume
HKR, Settings, "VidM", 1, 01     ;   Video Volume

HKR, Settings, "AuxV", 1, 08     ;   Aux Volume
HKR, Settings, "AuxM", 1, 01     ;   Aux Mute

HKR, Settings, "20db", 1, 00     ;   Mic 20db Gain (disable gain = 0)
HKR, Settings, "MicV", 1, 08     ;   Mic In Volume
HKR, Settings, "MicM", 1, 01     ;   Mic In Mute
HKR, Settings, "MicS", 1, 00     ;   Mic In Select (0 == Mic1, 1 == Mic2)

HKR, Settings, "ACDV", 1, 08     ;   Analog CD Volume (not digital redbook !)
HKR, Settings, "ACDM", 1, 00     ;   Analog CD Mute

HKR, Settings, "P3DV", 1, 0A     ;   Stereo Wide (Phat 3D) Volume ( 0 - F )
HKR, Settings, "P3DM", 1, 00     ;   Phat 3D Mute
HKR, Settings, "P3DB", 1, 01     ;   Use enhancement on digital streams

HKR, Settings, "MonV", 1, 08     ;   Mono Out Volume
HKR, Settings, "MonM", 1, 01     ;   Mono Out Mute
HKR, Settings, "RecS", 1, 00     ;   Record source (0=Mic, 1=CD, 2=Vid, 3=Aux
                                 ;      4=LineIn, 5=WaveOut, 6=MonoOut, 7=Phone

HKR, Settings, "HP_V", 1, 08     ;   Headphone Volume
HKR, Settings, "HP_M", 1, 00     ;   Headphone Mute



; Record Controls

HKR, Settings, "MicR", 1, 08     ;   Mic
HKR, Settings, "ACDR", 1, 01     ;   CD (Analog CD, not Redbook Audio)
HKR, Settings, "VidR", 1, 01     ;   Video
HKR, Settings, "AuxR", 1, 01     ;   Aux
HKR, Settings, "LinR", 1, 01     ;   Line In
HKR, Settings, "OutR", 1, 00     ;   Line output loopback
HKR, Settings, "MonR", 1, 01     ;   Mono output loopback
HKR, Settings, "PhoR", 1, 01     ;   Phone

; Enable Interrupt on each processed BDL
;  00 = Interrupt only when KMixer request
;  01 = Interrupt on every BDL
HKR, Settings, "SGUpdate", 1, 01

; Disable Node display on mixer applet. Set to 00 to enable, 01 to disable.
HKR, Disable, "NULL", 1, 00     ;   Generic handler for un-named nodes
HKR, Disable, "PCBV", 1, 01     ;   PCBeep Volume
HKR, Disable, "PCBM", 1, 01     ;   PCBeep Mute
HKR, Disable, "PhoV", 1, 00     ;   Phone Volume
HKR, Disable, "PhoM", 1, 00     ;   Phone Mute
HKR, Disable, "LinV", 1, 00     ;   LineIn Volume
HKR, Disable, "LinM", 1, 00     ;   LineIn Mute
HKR, Disable, "VidV", 1, 00     ;   Video Volume
HKR, Disable, "VidM", 1, 00     ;   Video Mute

HKR, Disable, "AuxV", 1, 00     ;   Aux Volume
HKR, Disable, "AuxM", 1, 00     ;   Aux Mute

HKR, Disable, "20db", 1, 00     ;   Mic 20db Gain
HKR, Disable, "MicV", 1, 00     ;   Mic In Volume
HKR, Disable, "MicM", 1, 00     ;   Mic In Mute
HKR, Disable, "MicS", 1, 00     ;   Mic In Select

HKR, Disable, "ACDV", 1, 00     ;   Analog CD Volume (not digital redbook !)
HKR, Disable, "ACDM", 1, 00     ;   Analog CD Mute

HKR, Disable, "P3DV", 1, 00     ;   Stereo Wide (Phat 3D) Volume
HKR, Disable, "P3DM", 1, 00     ;   Phat 3D Mute
HKR, Disable, "P3DB", 1, 00     ;   Phat 3D Bypass for digital streams
HKR, Disable, "MonV", 1, 00     ;   Mono Out Volume
HKR, Disable, "MonM", 1, 00     ;   Mono Out Mute
; Record Controls
HKR, Disable, "MicR", 1, 00     ;   Mic
HKR, Disable, "ACDR", 1, 00     ;   CD (Analog CD, not Redbook Audio)
HKR, Disable, "VidR", 1, 00     ;   Video
HKR, Disable, "AuxR", 1, 00     ;   Aux
HKR, Disable, "LinR", 1, 00     ;   Line In
HKR, Disable, "OutR", 1, 00     ;   Line output loopback
HKR, Disable, "MonR", 1, 01     ;   Mono output loopback
HKR, Disable, "PhoR", 1, 01     ;   Phone

;If you want the MonoOut to track the Master Volume control, set MonoWithMaster
;to 01. If you want separate Master Volume and MonoOut controls, set
;MonoWithMaster to 00. If MonoWithMaster = 01, the "MonoOut" controls will _not_
;be present on SndVol32 (the Master Volume control will control the MonoOut
;output)
HKR, Settings, "MonoWithMaster", 1, 00 ;   00 = Normal, 01 = MonoOut tracks Master

;If a AD1885 is detected and you want the (headphone) amplifier to track the
;Master Volume control, set HPWithMaster to 01. If you want separate controls
;for the Master Volume and Headphone, set HPWithMaster to 00. If
;HpWithMaster = 01, the "Headphone" controls will _not_ be present on SndVol32
;(the Master Volume control will control the Headphone amplifier output)
HKR, Settings, "HPWithMaster", 1, 01 ;   00 = Normal, 01 = Amplifier output tracks Master

;If a AD1885 is detected and the (headphone) amplifier is used, set HP_P to 00.
;If the amplified output is not used, set HP_P to 01. If you selected
;HPWithMaster, this setting is interpreted to be 01 (not active).
HKR, Disable, "HP_P", 1, 00     ;   Headphone Pin (Headphone destination active on 1885's)
                                ;    00 = active, 01 = not active

[NoCrystal.AddReg]
; Enable support for hardware designs that do not use a crystal to
;  geterate the AC'97 link bit clock.
;  00 = Use crystal/normal bit clock
;  01 = Use other clock for bit clock
; The values used here assume a 14.31818 MHz bit clock (28.63636 XTAL)
HKR, Settings, "NoCrystal", 1, 01
HKR, Settings, "48000", 1, EA, A0, 00, 00
HKR, Settings, "44100", 1, D7, 93, 00, 00
HKR, Settings, "32000", 1, 46, 6B, 00, 00
HKR, Settings, "24000", 1, 75, 50, 00, 00
HKR, Settings, "22050", 1, EB, 49, 00, 00
HKR, Settings, "16000", 1, A3, 35, 00, 00
HKR, Settings, "12000", 1, 3A, 28, 00, 00
HKR, Settings, "11025", 1, F5, 24, 00, 00
HKR, Settings, "8000", 1, D1, 1A, 00, 00





[WDM_ICHAUD_GUID.AddReg]
HKLM,%MediaCategories%\%ADIGUID.PcBeep%,Name,,%Pin.PcBeep%
HKLM,%MediaCategories%\%ADIGUID.PcBeep%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Phone%,Name,,%Pin.Phone%
HKLM,%MediaCategories%\%ADIGUID.Phone%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Video%,Name,,%Pin.Video%
HKLM,%MediaCategories%\%ADIGUID.Video%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MonoOut%,Name,,%Pin.MonoOut%
HKLM,%MediaCategories%\%ADIGUID.MonoOut%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.PCBeepVol%,Name,,%Control.PCBeepVol%
HKLM,%MediaCategories%\%ADIGUID.PCBeepVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.PhoneVol%,Name,,%Control.PhoneVol%
HKLM,%MediaCategories%\%ADIGUID.PhoneVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.VIDVol%,Name,,%Control.VIDVol%
HKLM,%MediaCategories%\%ADIGUID.VIDVol%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.20DB%,Name,,%Control.20DB%
HKLM,%MediaCategories%\%ADIGUID.20DB%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.PHATBypass%,Name,,%Control.PHATBypass%
HKLM,%MediaCategories%\%ADIGUID.PHATBypass%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MonoVol%,Name,,%Control.MonoVol%
HKLM,%MediaCategories%\%ADIGUID.MonoVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MicSelect%,Name,,%Control.MicSelect%
HKLM,%MediaCategories%\%ADIGUID.MicSelect%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.CaptureVid%,Name,,%Control.CaptureVid%
HKLM,%MediaCategories%\%ADIGUID.CaptureVid%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CaptureMono%,Name,,%Control.CaptureMono%
HKLM,%MediaCategories%\%ADIGUID.CaptureMono%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CapturePhone%,Name,,%Control.CapturePhone%
HKLM,%MediaCategories%\%ADIGUID.CapturePhone%,Display,1,00,00,00,00

[DriverInfo.AddReg]
; This section is added to all INFs to add registry entries for Driver Information.
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileName,,%BaseDriverFileName%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileVersion,,%BaseDriverFileVersion%

[SourceDisksNames.x86]
222=%Empty%,,,

[SourceDisksFiles.x86]
;smx.cat=222
smwdm.sys=222

;; Delete these files from
;; the system directory
[system.DelFiles]
ichaudio.sys
ichaud.sys
smwdm.sys

;; copy these files into the
;; system32\drivers directory
[WDM_ICHAUD.CopyList]
smwdm.sys


;;**************** NT Install ****************

[WDM_ICHAUD.NT]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_ICHAUD.CopyList
DelFiles=system.DelFiles
AddReg=WDM_ICHAUD.AddReg, WDM_ICHAUD_GUID.AddReg, DriverInfo.AddReg

[WDM_ICHAUD.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, ICHAud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, ICHAud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, ICHAud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, ICHAud.Interface.Topology

[ICHAud.Interface.Wave]
AddReg=ICHAud.Interface.Wave.AddReg
[ICHAud.Interface.Wave.AddReg]
HKR,,FriendlyName,,%ICHAud.Wave.szPname%
HKR,,CLSID,,%Proxy.CLSID%

[ICHAud.Interface.Topology]
AddReg=ICHAud.Interface.Topo.AddReg
;;must use topo because topology is too long
[ICHAud.Interface.Topo.AddReg]
HKR,,FriendlyName,,%ICHAud.Topology.szPname%

[WDM_ICHAUD.NT.Services]
AddService = smwdm, 0x00000002, WDM_ICHAUD_Service_Inst

[WDM_ICHAUD_Service_Inst]
;DisplayName    = %WDM_ICHAUD.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\system32\drivers\smwdm.sys

[Strings]
;; AC'97 Device friendly names (GUIDS non-localizeable)

ADIGUID.PcBeep      ="{992C6360-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MonoOut     ="{992C6361-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Phone       ="{992C6362-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Video       ="{992C6366-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PCBeepVol   ="{992C6372-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MonoVol     ="{992C6374-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PhoneVol    ="{992C6376-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.VIDVol      ="{992C637A-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.20DB        ="{992C6380-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PHATBypass  ="{992C6387-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MicSelect   ="{992C638D-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.CaptureVid  ="{992C6392-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CaptureMono ="{992C6396-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CapturePhone ="{992C6397-643D-11D2-9BDC-00A0C9696B7D}"

;; Analog Devices friendly names (localizeable)
;Sources (Pins)
Pin.PcBeep       ="PC Beep"          ; PC Beep Input
Pin.MonoOut      ="Mono Out"         ; Mono line output
Pin.Phone        ="Phone"            ; Phone Input
Pin.Video        ="Video"            ; Video Input

;Controls       (Controls as related to Sources)

Control.PCBeepVol     ="PCBeep Volume"   ; PC Beep volume control name
Control.PhoneVol      ="Phone Volume"    ; Phone volume control name
Control.VIDVol        ="Video Volume"    ; Video volume control name
Control.20DB          ="+20db Gain"       ; Microphone advanced control
Control.PHATBypass    ="Apply 3D effect to digital audio"
                                         ; 3D bypass control string (bypass
                                         ;  spatialization on digital streams)

Control.MonoVol       ="Mono Volume"     ; Monoaural Output volume control name
Control.MicSelect     ="Mic2 Select"     ; Microphone advanced control

Control.CaptureVid    ="Video"           ; Video Record
Control.CaptureMono   ="Mono Out"        ; Mono Mix Record
Control.CapturePhone  ="Phone"           ; Phone Record

MediaCategories="SYSTEM\CurrentControlSet\Control\MediaCategories"
WDM_MIDI="WDM-based Device"
Proxy.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_AUDIO="{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_RENDER="{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSNAME_Wave="Wave"
KSNAME_Topology="Topology"

ANLG="Analog Devices"
MfgName="Analog Devices, Inc."
Empty=""

*WDM_ICHAUD.DeviceDesc="SoundMAX Integrated Digital Audio"
ICHAud.Wave.szPname="SoundMAX Digital Audio"
ICHAud.Topology.szPname="SoundMAX Digital Audio"

;WDM_ICHAUD.SvcDesc = "SoundMAX Integrated Digital Audio"

; History Information
DriverMfgr="AnalogDevices"
DriverVersionID="5.12.2502"
DriverOEM="AnalogDevices"
DriverFamily="Audio"
DriverProduct="SoundMAX"
DriverDescription="Audio Driver"
DriverOEMVersion="x00"
BaseDriverFileName="smwdm.sys"
BaseDriverFileVersion="5.12.2502"
